Standard Firmware Version
##################################

Printer:	T2150 / T2250 / T2150S

Id:		70363
Index:		A
Date:		12. August 2013
ECN:		20775-02

Development:	DEU

Based on:	70363
Index:		-



A) Functional changes

1. Epson(R) EJL string is now ignored:
The initial Epson(R) driver string for ESC/P2 printers ("@EJL 1284.4<0A>@EJL<20 20 20 20 20 0A>")
will be ignored. This is to establish compatibility to current LQ drivers,
Set printer to LQ-2170 emulation in this case!

2. Extended parameter for MTPL command 'ESC [ <n1> ; <n2> {':
The parameter <n2> of the MTPL sequence which sets the vertical alignment,
can now have an extended value of max. 60/72” (was max. 40/72” before).

3. Changed the time used for monitoring the cutting process (HWA):
Changed the time until ‘Hardware Alarm’ is reported during a cutting process from 550 ms
to 750 ms because of problems reported with a few cutters.

4. Changed the regulation of the horizontal motor:
The functionality of the horizontal motor was adapted to the properties of a new CR motor.
This change is backwards compatible with the previous motor.


B) Functional improvements and bug fixes

1. Fixed a problem in the printer’s test menu:
In the test menu, when the 3rd submenu of “Paphand” was selected and then key 3
(with no text above) was pressed, the printer showed “HDW Trap” on the panel.

2. Fixed a problem with Ethernet Interface:
In some rare circumstances the printer was catched in a endless loop with resets. Solved.


(c) DASCOM Europe GmbH
EMEA Technical Support
DEU/PTS - fs
8'2013
All rights reserved