Firmware for Thermal Printers 
~~~~~~~~~~
Date:		Jan 2013
Name:		DS400300.s4e
Printer:	7106 & 7206
DPI:		300
Reason:		Motor control improved


Question
~~~~~~~~~~
How to load firmware in 7x06 and 7010?

Answer
~~~~~~~~~~
Just copy it to the printer using any interface.

Consider
~~~~~~~~~~
DASCOM does NOT take any responsibility for damaging printer caused by improper flashing of fimrware!

For instance:
~~~~~~~~~~

- USB
Install a driver and send the file over this port

- Serial
Copy/b firmware com1:

- Parallel
Copy/b firmware prn:

- Ethernet
Install a driver and send the file over this ethernet ip port

IMPORTANT
~~~~~~~~~~
Wait until the printer beeps shortly. Otherwise you may damage the printer!
Also, here is a tip of information for your reference.
When you write F/W you are actually doing this -->.
a. forwarding F/W data to the printer
b. processing the data at the memory
c. deleting the data within the memory by block unit d. re-writing F/W data by block unit

If the printer turn off the power white deleting (above c), a part of memory will be empty
and the printer does not operate properly.



(c) DASCOM Europe GmbH
DEU/TS - fs
EMEA Technical Support
November 2013
All rights reserved
